SN74151:

This chip is binary to one hot decoder. When En (Not G) =1, this decoder translates 3-bit binary code to one-hot code.

SN74154:

This chip is also binary to one hot code decoder. EN is Not (G1 OR G2). When EN = 1, this decoder will translate 4-bit binary code to one-hot code.